# TKE_Color_Map

## Opcode

ASCII | (none)
Hexadecimal | 0C
Decimal | 12

## Operands

Byte format, Long length,
if format = 0:
(3xlength)xByte rgbs

format | type of color map definition, currently only format 0 (RGB triplets) is defined
rgbs | length triplets, RGB color components in the range 0-255

## Notes

A color map is a lookup to convert an index (ie, Color_By_Index or mapped image) into a color definition.