# TKE_Priority

## Opcode

ASCII | 0
Hexadecimal | 30
Decimal | 48

## Operands

Long value

value | priority to be associated with the object

## Notes

This opcode allows the user to specify a priority value to associate with subsegments and includes. This value overrides the default alphabetical sorting order, so that the drawing order of sibling segments may be directly controlled (higher values are visited later).