===================
TKE_Include_Segment
===================

Opcode
======

.. csv-table::

	"ASCII", "<"
	"Hexadecimal", "3C"
	"Decimal", "60"


Operands
========

Byte flag_or_length, [Byte length,] (length)xByte name 
[Byte condition_length, (condition_length)xByte condition]

.. csv-table::

	"flag_or_length", "If not 0, the length of the segment name string. If 0, the length follows immediately, and the condition fields follow the segment name."
	"length", "length of the segment name string"
	"name", "name of the segment to be included"
	"condition_length", "length of the condition string"
	"condition", "logical test based on condition flags"
	
	
Notes
=====

The specified segment is to "included" in the current segment; it is drawn as if it were a local subsegment. Included segment are used to instance objects within your scene graph. If a condition is present, it must evaluate to true before the segment is processed.

Conditions and flagging the length were added in HSF version 11.50.
