:orphan:

===============
TKE_Local_Light
===============

Opcode
======

.. csv-table::

	"ASCII", "."
	"Hexadecimal", "2E"
	"Decimal", "46"


Operands
========

| Point position
| byte options 

.. csv-table::

	"position", "location of the point light"
	"options", "flags to indicate optional attributes attached to the light"
	
	
Optional attributes for TKE_Local_Light
---------------------------------------

.. csv-table::

	"0x01", "Camera-relative. Instead of an object-space position, position is relative to the camera location instead of the origin."


Notes
=====

Onmi-directional "point" source of light is inserted into the currently opened segment.
