:orphan:

=================
TKE_Distant_Light
=================

Opcode
======

.. csv-table::

	"ASCII", "d"
	"Hexadecimal", "64"
	"Decimal", "100"


Operands
========

| Point direction
| byte options 

.. csv-table::
	
	"direction", "vector towards the light"
	"options", "flags to indicate optional attributes attached to the light"
	
	
Optional attributes for TKE_Distant_Light
-----------------------------------------

.. csv-table::

	"0x01", "Camera-relative. Direction vector is relative to the camera direction. A value of <0,0,-1> corresponds to a light along the same direction as the camera."
	

Notes
=====

Light is inserted into the currently opened segment.
