# Flags for Specifying Wire Characteristics

Bitmasks used in the `A3DTess3DWireData`structure to describe wire characteristics.

> 2.0

These bitmasks must be applied on the first unsigned int containing the number of related indexes in the array used to described current wire.

## Index

Preprocessor Definitions

- `kA3DTess3DWireDataIsClosing`
- `kA3DTess3DWireDataIsContinuous`

Preprocessor Definitions

`kA3DTess3DWireDataIsClosing`

  The current wire is closed.

`kA3DTess3DWireDataIsContinuous`

  Indicates that the last point of preceding wire should be linked with the first point of the current one.

Conversation saved
HOOPSY BETA

### Hello! I'm HOOPSY

Your multilingual generative AI assistant for documentation. Ask me anything about HOOPS Exchange in your own language, or choose a sample question below to start a conversation:

What is HOOPS Exchange?
What are the latest release notes for HOOPS Exchange?
How do I start evaluating HOOPS Exchange?
How do I write my first sample application?
How can I get assistance?

HOOPSY may store conversations according to OpenAI's policy. Responses may not always be accurate.

HOOPSY is thinking...