
#########################
A3DCollisionParameterData
#########################

.. c:struct:: A3DCollisionParameterData

   :c:struct:`~A3DCollisionParameterData`\ structure.
   
   
      11.1
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DCollisionParameterData.m_dSafetyDistance`
   * :c:member:`~A3DCollisionParameterData.m_dContactLimit`
   * :c:member:`~A3DCollisionParameterData.m_dTessellationTolerance`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DDouble A3DCollisionParameterData.m_dSafetyDistance

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      It makes possible to identify parts between which a specified distance is not verified.
      
      The safety distance value has to be greater than :c:member:`m_dContactLimit <A3DCollisionParameterData.m_dContactLimit>`
      



.. c:member:: A3DDouble A3DCollisionParameterData.m_dContactLimit

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      This value defines the upper limit of distances interval in which the parts are judged "in contact".
      
      The minimum value for the contact limit 0.1 mm, or can be set to 0. to check only clearance and collision cases.
      



.. c:member:: A3DDouble A3DCollisionParameterData.m_dTessellationTolerance

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Computation tolerance.
      
      The minimal value is 0.01 mm. The tolerance value cannot be greater than :c:member:`m_dContactLimit <A3DCollisionParameterData.m_dContactLimit>`\ .
      




