
###############################
A3DAsmModelFileLoadFromPRCFiles
###############################

.. c:function:: A3DStatus A3DAsmModelFileLoadFromPRCFiles(const A3DUTF8Char *pcRootPrcFilePath, const A3DUns32 uNbFile, const A3DUTF8Char **ppPRCFilePath, const A3DUTF8Char **ppCADFilePath, const A3DRWParamsLoadData *pParamsLoadData, A3DAsmModelFile **pA3DAsmModelFile)

   .. rst-class:: sig-pretty-signature
   
      | :c:enum:`~A3DStatus` A3DAsmModelFileLoadFromPRCFiles(*const* :c:type:`~A3DUTF8Char`\ \* **pcRootPrcFilePath**\ , *const* :c:type:`~A3DUns32` **uNbFile**\ , *const* :c:type:`~A3DUTF8Char`\ \*\* **ppPRCFilePath**\ , *const* :c:type:`~A3DUTF8Char`\ \*\* **ppCADFilePath**\ , *const* :c:struct:`~A3DRWParamsLoadData`\ \* **pParamsLoadData**\ , :c:type:`~A3DAsmModelFile`\ \*\* **pA3DAsmModelFile**\ )
   
   Creates a model file from multiple PRC files + a PRC assembly file + a map for file names.
   
   This function inserts all the parts and product occurrences from a file list into a single PRC assembly file loaded in "assembly NO Dependency" mode and outputs a reassembled model file.
   
   **Parameters**
   
   
      **pcRootPrcFilePath**\ : The file name of the top assembly file. This model file is loaded as assembly tree only and saved as a PRC file.
   
      **uNbFile**\ : The number of file names to plug into the assembly.
   
      **ppPRCFilePath**\ : The equivalent PRC file paths for parts. Length must equal uNbFile.
   
      **ppCADFilePath**\ : The native part file paths. Length must equal uNbFile.
   
      **pParamsLoadData**\ : The parameters to use when reading the model files. Configuration must be set to read the default entry or must only specify a single entry to read.
   
      **pA3DAsmModelFile**\ : The final reassembled model file.
   
   
   **Returns**
   
   
      ``A3D_SUCCESS``\ on success, or an error code on failure
   
   




