
########################
A3DDrawingFilledAreaData
########################

.. c:struct:: A3DDrawingFilledAreaData

   DrawingFilledArea structure.
   
   
      5.0
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DDrawingFilledAreaData.m_eMode`
   * :c:member:`~A3DDrawingFilledAreaData.m_uiPatternIndex`
   * :c:member:`~A3DDrawingFilledAreaData.m_bIgnoreViewTransfo`
   * :c:member:`~A3DDrawingFilledAreaData.m_uiBoundaryCurvesSize`
   * :c:member:`~A3DDrawingFilledAreaData.m_ppBoundaryCurves`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DEDrawingFilledAreaMode A3DDrawingFilledAreaData.m_eMode

      .. rst-class:: sig-pretty-signature
      
         | :c:enum:`~A3DEDrawingFilledAreaMode`
      
      Fill mode refers to :c:enum:`~A3DEDrawingFilledAreaMode`\ for more details.
      



.. c:member:: A3DUns32 A3DDrawingFilledAreaData.m_uiPatternIndex

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DUns32`
      
      Pattern index.
      
      Refers to :ref:`Graphics <group__a3d__graphics__module>`\ for more details.
      



.. c:member:: A3DBool A3DDrawingFilledAreaData.m_bIgnoreViewTransfo

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Indiquate if drawing of pattern is independent of view transformation.
      
      
      



.. c:member:: A3DUns32 A3DDrawingFilledAreaData.m_uiBoundaryCurvesSize

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DUns32`
      
      The size of :c:member:`m_ppBoundaryCurves <A3DDrawingFilledAreaData.m_ppBoundaryCurves>`\ .
      



.. c:member:: A3DCrvBase** A3DDrawingFilledAreaData.m_ppBoundaryCurves

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DCrvBase`\ \*\*
      
      Array of closed curves.
      
      Refers to :ref:`Curves Module <group__a3d__crv>`\ for more details Each curve must be closed. Intersection area is processed with m_eMode parameter.
      




