
############################
A3DMiscMaterialIsotropicData
############################

.. c:struct:: A3DMiscMaterialIsotropicData

   Isotropic physical properties.
   
   
      9.0
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dYoungModulus`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dPoissonRatio`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dShearModulus`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dThermalExpansion`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dThermalConductivity`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dSpecificHeat`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dYieldStrength`
   * :c:member:`~A3DMiscMaterialIsotropicData.m_dTensileStrength`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dYoungModulus

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Young Modulus in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dPoissonRatio

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Poisson Ratio (unitless).
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dShearModulus

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Modulus in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dThermalExpansion

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Thermal Expansion Coefficient in 1/K.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dThermalConductivity

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Thermal Conductivity in W/(m.K).
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dSpecificHeat

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Specific Heat in J/(kg.K).
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dYieldStrength

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Yield Strength in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialIsotropicData.m_dTensileStrength

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Tensile Strength in Pa.
      
      Equal to -1.0 if not set
      




