
####################
A3DECompressBrepType
####################

.. c:enum:: A3DECompressBrepType

   Level of compression used to write the model file to PRC format.
   
   This sets the amount, in millimeters, of lossy compression that is applied to geometry. For best results when exporting geometry, use kA3DCompressionLow.
   
   
      3.0
   
   
   
   Index
   =====
   
   .. rubric:: Enumerators
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:enumerator:`~kA3DCompressionLow`
   * :c:enumerator:`~kA3DCompressionMedium`
   * :c:enumerator:`~kA3DCompressionHigh`
   
   



.. rst-class:: kind-group kind-enumerator

.. rubric:: Enumerators
   :class: kind-group-title


.. c:enumerator:: kA3DCompressionLow

      .. rst-class:: sig-pretty-signature
      
         | **kA3DCompressionLow** = ``0``
      
      Compression with tolerance set to 0.001 mm (low compression, high accuracy).
      



.. c:enumerator:: kA3DCompressionMedium

      .. rst-class:: sig-pretty-signature
      
         | **kA3DCompressionMedium**
      
      Compression with tolerance set to 0.01 mm (medium compression, medium accuracy).
      



.. c:enumerator:: kA3DCompressionHigh

      .. rst-class:: sig-pretty-signature
      
         | **kA3DCompressionHigh**
      
      Compression with tolerance set to 0.1 mm (high compression, low accuracy).
      




