
#########################
A3DRWParamsExportAcisData
#########################

.. c:struct:: A3DRWParamsExportAcisData

   A structure that specifies parameters used to write the model file to ACIS format.
   
   
      4.2
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DRWParamsExportAcisData.m_bSaveAsMillimeter`
   * :c:member:`~A3DRWParamsExportAcisData.m_bSaveAsBinary`
   * :c:member:`~A3DRWParamsExportAcisData.m_bForceSurfaceDuplication`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DBool A3DRWParamsExportAcisData.m_bSaveAsMillimeter

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Save data in millimeter instead of current model unit.
      



.. c:member:: A3DBool A3DRWParamsExportAcisData.m_bSaveAsBinary

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Save in binary file (.sab).
      



.. c:member:: A3DBool A3DRWParamsExportAcisData.m_bForceSurfaceDuplication

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Force surface duplication -:c:type:`~A3DSurfBase`\ are not shared between :c:type:`~A3DTopoFace`\ .
      




