
########################
A3DMiscMaterialFiberData
########################

.. c:struct:: A3DMiscMaterialFiberData

   Fiber physical properties.
   
   
      9.0
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DMiscMaterialFiberData.m_dYoungModulus_X`
   * :c:member:`~A3DMiscMaterialFiberData.m_dYoungModulus_Y`
   * :c:member:`~A3DMiscMaterialFiberData.m_dPoissonRatio_XY`
   * :c:member:`~A3DMiscMaterialFiberData.m_dShearModulus_XY`
   * :c:member:`~A3DMiscMaterialFiberData.m_dShearModulus_YZ`
   * :c:member:`~A3DMiscMaterialFiberData.m_dThermalExpansion_X`
   * :c:member:`~A3DMiscMaterialFiberData.m_dThermalExpansion_Y`
   * :c:member:`~A3DMiscMaterialFiberData.m_dTensileStressLimit_X`
   * :c:member:`~A3DMiscMaterialFiberData.m_dCompressiveStressLimit_X`
   * :c:member:`~A3DMiscMaterialFiberData.m_dTensileStressLimit_Y`
   * :c:member:`~A3DMiscMaterialFiberData.m_dCompressiveStressLimit_Y`
   * :c:member:`~A3DMiscMaterialFiberData.m_dShearStressLimit_XY`
   * :c:member:`~A3DMiscMaterialFiberData.m_dShearStressLimit_YZ`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dYoungModulus_X

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Longitudinal Young Modulus in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dYoungModulus_Y

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Transverse Young Modulus in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dPoissonRatio_XY

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Poisson Ratio in XY plane.
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dShearModulus_XY

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Modulus in XY plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dShearModulus_YZ

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Modulus in XZ plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dThermalExpansion_X

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Longitudinal Thermal Expansion Coefficient in 1/K.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dThermalExpansion_Y

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Transverse Thermal Expansion Coefficient in 1/K.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dTensileStressLimit_X

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Longitudinal Tensile Stress Limit in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dCompressiveStressLimit_X

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Longitudinal Compressive Stress Limit in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dTensileStressLimit_Y

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Transverse Tensile Stress Limit in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dCompressiveStressLimit_Y

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Transverse Compressive Stress Limit in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dShearStressLimit_XY

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Stress Limit in XY plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialFiberData.m_dShearStressLimit_YZ

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Stress Limit in XZ plane in Pa.
      
      Equal to -1.0 if not set
      




