# Export SCS Module

(HOOPS Publish Advanced)Structure and function to write a ModelFile as a SCS stream cache file.

SCS is the Stream Cache Single file format used in HOOPS Communicator to hold the representation of a CAD model. A SCS file is later expected to be referred by a HTML file. This format stores the tessellated geometry, the assembly tree and all non-tessellation related data: PMI, views, user attributes, etc. Also, exact measurement data can be optionally added to the SCS file to store geometrical information useful for measurement tool, such as cylinder and radius data on faces or edges. This measurement information can take time to be computed and should only be added on purpose to handle measurement scenarios.

Parameters

> pA3DAsmModelFile: References The `A3DAsmModelFile`to be exported

> pParamsExportData: References the parameters for export.

> pcScsFileName: References the path of the file into which the function stores the model file.

Returns

> A3D_SUCCESS in case of success or an error code

Structures

- `deprecated_A3DRWParamsExportScsData`

Functions

- `deprecated_A3DAsmModelFileExportToSCSFile()`

Conversation saved
HOOPSY BETA

### Hello! I'm HOOPSY

Your multilingual generative AI assistant for documentation. Ask me anything about HOOPS Exchange in your own language, or choose a sample question below to start a conversation:

What is HOOPS Exchange?
What are the latest release notes for HOOPS Exchange?
How do I start evaluating HOOPS Exchange?
How do I write my first sample application?
How can I get assistance?

HOOPSY may store conversations according to OpenAI's policy. Responses may not always be accurate.

HOOPSY is thinking...