
##############################
A3DAsmProductOccurrenceDataCV5
##############################

.. c:struct:: A3DAsmProductOccurrenceDataCV5

   A structure specifying the product occurrence data specific to the CV5 format.
   
   
      8.2
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_psRootFilePath`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_iRootModificationTime`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_iRootUpdateIndex`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_iCurrentAsmProductIdentifier`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_iNotUpdatedAsmProductIdentifier`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_aiCLSID`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_bProductInError`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_bHasCGMInformation`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_bFromCATPart`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_psVersion`
   * :c:member:`~A3DAsmProductOccurrenceDataCV5.m_psPartNumber`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DUTF8Char* A3DAsmProductOccurrenceDataCV5.m_psRootFilePath

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DUTF8Char`\ \*
      
      unique ID : to be sure incremental loading is ok, we need the same root assembly file with same timestamp.
      
      Otherwise : must reload all.
      



.. c:member:: A3DInt32 A3DAsmProductOccurrenceDataCV5.m_iRootModificationTime

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DInt32`
      
      Root file modification time.
      



.. c:member:: A3DInt32 A3DAsmProductOccurrenceDataCV5.m_iRootUpdateIndex

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DInt32`
      
      Root file update index.
      



.. c:member:: A3DInt32 A3DAsmProductOccurrenceDataCV5.m_iCurrentAsmProductIdentifier

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DInt32`
      
      Current assembly product identifier.
      



.. c:member:: A3DInt32 A3DAsmProductOccurrenceDataCV5.m_iNotUpdatedAsmProductIdentifier

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DInt32`
      
      Not updated assembly product identifier.
      



.. c:member:: A3DInt32 A3DAsmProductOccurrenceDataCV5.m_aiCLSID[4]

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DInt32`
      
      CLSID array.
      



.. c:member:: A3DBool A3DAsmProductOccurrenceDataCV5.m_bProductInError

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Indicates if the product is in error state.
      



.. c:member:: A3DBool A3DAsmProductOccurrenceDataCV5.m_bHasCGMInformation

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Indicates if CGM information is present.
      



.. c:member:: A3DBool A3DAsmProductOccurrenceDataCV5.m_bFromCATPart

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DBool`
      
      Indicates if from CATPart.
      



.. c:member:: A3DUTF8Char* A3DAsmProductOccurrenceDataCV5.m_psVersion

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DUTF8Char`\ \*
      
      Version string.
      



.. c:member:: A3DUTF8Char* A3DAsmProductOccurrenceDataCV5.m_psPartNumber

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DUTF8Char`\ \*
      
      Part number string.
      




