
############################
A3DMiscMaterialHoneyCombData
############################

.. c:struct:: A3DMiscMaterialHoneyCombData

   HoneyComb physical properties.
   
   
      9.0
   
   
   
   Index
   =====
   
   .. rubric:: Variables
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:member:`~A3DMiscMaterialHoneyCombData.m_dYoungModulus`
   * :c:member:`~A3DMiscMaterialHoneyCombData.m_dShearModulus_XZ`
   * :c:member:`~A3DMiscMaterialHoneyCombData.m_dShearModulus_YZ`
   * :c:member:`~A3DMiscMaterialHoneyCombData.m_dShearStressLimit_XZ`
   * :c:member:`~A3DMiscMaterialHoneyCombData.m_dShearStressLimit_YZ`
   * :c:member:`~A3DMiscMaterialHoneyCombData.m_dThermalExpansion`
   
   



.. rst-class:: kind-group kind-variable

.. rubric:: Variables
   :class: kind-group-title


.. c:member:: A3DDouble A3DMiscMaterialHoneyCombData.m_dYoungModulus

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Normal Young Modulus in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialHoneyCombData.m_dShearModulus_XZ

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Modulus in XY plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialHoneyCombData.m_dShearModulus_YZ

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Modulus in XZ plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialHoneyCombData.m_dShearStressLimit_XZ

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Stress Limit in XY plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialHoneyCombData.m_dShearStressLimit_YZ

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Shear Stress Limit in XZ plane in Pa.
      
      Equal to -1.0 if not set
      



.. c:member:: A3DDouble A3DMiscMaterialHoneyCombData.m_dThermalExpansion

      .. rst-class:: sig-pretty-signature
      
         | :c:type:`~A3DDouble`
      
      Normal Thermal Expansion Coefficient in 1/K.
      
      Equal to -1.0 if not set
      




