
###################
A3DEMDRoughnessMode
###################

.. c:enum:: A3DEMDRoughnessMode

   Enumerator that describes the direction of lay.
   
   
   Index
   =====
   
   .. rubric:: Enumerators
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:enumerator:`~kA3DRoughnessMode_None`
   * :c:enumerator:`~kA3DRoughnessModeM`
   * :c:enumerator:`~kA3DRoughnessModeC`
   * :c:enumerator:`~kA3DRoughnessModeR`
   * :c:enumerator:`~kA3DRoughnessModeP`
   * :c:enumerator:`~kA3DRoughnessModeX`
   * :c:enumerator:`~kA3DRoughnessModePARA`
   * :c:enumerator:`~kA3DRoughnessModePERP`
   
   



.. rst-class:: kind-group kind-enumerator

.. rubric:: Enumerators
   :class: kind-group-title


.. c:enumerator:: kA3DRoughnessMode_None

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessMode_None** = ``0``
      
      No specified lay.
      



.. c:enumerator:: kA3DRoughnessModeM

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModeM** = ``1``
      
      Lay multi directional.
      



.. c:enumerator:: kA3DRoughnessModeC

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModeC** = ``2``
      
      Lay approximately circular.
      



.. c:enumerator:: kA3DRoughnessModeR

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModeR** = ``3``
      
      Lay approximately radial.
      



.. c:enumerator:: kA3DRoughnessModeP

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModeP** = ``4``
      
      Lay particulate, non-directional, or protuberant.
      



.. c:enumerator:: kA3DRoughnessModeX

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModeX** = ``5``
      
      Lay angular in both directions.
      



.. c:enumerator:: kA3DRoughnessModePARA

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModePARA** = ``6``
      
      Lay approximately parallel to the line representing the surface.
      



.. c:enumerator:: kA3DRoughnessModePERP

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRoughnessModePERP** = ``7``
      
      Lay approximately perpendicular to the line representing the surface.
      




