
###################
A3DEReadingMode2D3D
###################

.. c:enum:: A3DEReadingMode2D3D

   This value determines if we load only 3D, only Drawings or both.
   
   Both only apply to DWG/DXF for the moment
   
   
      12.0
   
   
   
   Index
   =====
   
   .. rubric:: Enumerators
   
   
   .. rst-class:: api-xref-list
   
   
   * :c:enumerator:`~kA3DRead_3D`
   * :c:enumerator:`~kA3DRead_Drawings`
   * :c:enumerator:`~kA3DRead_Both`
   
   



.. rst-class:: kind-group kind-enumerator

.. rubric:: Enumerators
   :class: kind-group-title


.. c:enumerator:: kA3DRead_3D

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRead_3D** = ``0``
      
      Read 3D Only.
      



.. c:enumerator:: kA3DRead_Drawings

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRead_Drawings** = ``1``
      
      Read Drawings only.
      



.. c:enumerator:: kA3DRead_Both

      .. rst-class:: sig-pretty-signature
      
         | **kA3DRead_Both** = ``2``
      
      Read 3D and Drawings.
      




