# A3DEFRMEnumValue_ChamferType

enum `A3DEFRMEnumValue_ChamferType`

  Enumerate the possible types of chamfer.

  This allow to specify the type of chamfer, and so the Definition you should expect to have under thekA3DFRMFeatureDefinitionType_Chamfer.

  > 11

  ## Index

  Enumerators

  - `kA3DFRMEnumValue_ChamferType_None`
  - `kA3DFRMEnumValue_ChamferType_Distance_Distance`
  - `kA3DFRMEnumValue_ChamferType_Distance1_Distance2`
  - `kA3DFRMEnumValue_ChamferType_Offset_Offset`
  - `kA3DFRMEnumValue_ChamferType_Offset1_Offset2`
  - `kA3DFRMEnumValue_ChamferType_Length_Angle`
  - `kA3DFRMEnumValue_ChamferType_ChordalLength_Angle`
  - `kA3DFRMEnumValue_ChamferType_Height_Angle`
  - `kA3DFRMEnumValue_ChamferType_Corner`

Enumerators

enumerator `kA3DFRMEnumValue_ChamferType_None`
  kA3DFRMEnumValue_ChamferType_None = `0`

  Invalid Chamfer Type.

enumerator `kA3DFRMEnumValue_ChamferType_Distance_Distance`
  kA3DFRMEnumValue_ChamferType_Distance_Distance

  Chamfer symmetric defined with one distance:

  - Value Length: chamfer length
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_Distance1_Distance2`
  kA3DFRMEnumValue_ChamferType_Distance1_Distance2

  Chamfer asymmetric defined with two distance:

  - Value Length: chamfer first distance
  - Value Length: chamfer second distance
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_Offset_Offset`
  kA3DFRMEnumValue_ChamferType_Offset_Offset

  Chamfer symmetric define with one distance:

  - Value Length: chamfer offset
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_Offset1_Offset2`
  kA3DFRMEnumValue_ChamferType_Offset1_Offset2

  Chamfer asymmetric defined with two distance:

  - Value Length: chamfer first offset
  - Value Length: chamfer second offset
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_Length_Angle`
  kA3DFRMEnumValue_ChamferType_Length_Angle

  Chamfer defined with one distance and an angle:

  - Value Length: chamfer length
  - Value Angle: chamfer angle
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_ChordalLength_Angle`
  kA3DFRMEnumValue_ChamferType_ChordalLength_Angle

  Chamfer defined with the chordal length and an angle:

  - Value Length: chamfer chordal length
  - Value Angle: chamfer angle
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_Height_Angle`
  kA3DFRMEnumValue_ChamferType_Height_Angle

  Chamfer defined with the distance between the edge and the new face and an angle:

  - Value Length: chamfer height
  - Value Angle: chamfer angle
  - Parameter Data:

enumerator `kA3DFRMEnumValue_ChamferType_Corner`
  kA3DFRMEnumValue_ChamferType_Corner

  Chamfer corner.

  Expect to have three chamfer definition with one length each:

  - Definition Chamfer: first chamfer definition
  - Definition Chamfer: second chamfer definition
  - Definition Chamfer: third chamfer definition
  - Parameter Definition:

Conversation saved
HOOPSY BETA

### Hello! I'm HOOPSY

Your multilingual generative AI assistant for documentation. Ask me anything about HOOPS Exchange in your own language, or choose a sample question below to start a conversation:

What is HOOPS Exchange?
What are the latest release notes for HOOPS Exchange?
How do I start evaluating HOOPS Exchange?
How do I write my first sample application?
How can I get assistance?

HOOPSY may store conversations according to OpenAI's policy. Responses may not always be accurate.

HOOPSY is thinking...